# Static Call Graph for image .\Objects\project.axf

#<CALLGRAPH># ARM Linker, 5060960: Last Updated: Tue Feb 25 12:23:32 2025

### Maximum Stack Usage = 108 bytes + Unknown(Functions without stacksize, Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

__rt_entry_main ⇒ main ⇒ HC05_Init ⇒ Serial_Init ⇒ USART_Init ⇒ RCC_GetClocksFreq

### Functions with no stack information

- __user_initial_stackheap

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(i.BusFault_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(i.DebugMon_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(i.HardFault_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(i.MemManage_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - NMI_Handler from stm32f10x_it.o(i.NMI_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(i.PendSV_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - Reset_Handler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - SVC_Handler from stm32f10x_it.o(i.SVC_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(i.SysTick_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - SystemInit from system_stm32f10x.o(i.SystemInit) referenced from startup_stm32f10x_md.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM2_IRQHandler from board_timer.o(i.TIM2_IRQHandler) referenced from startup_stm32f10x_md.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART1_IRQHandler from serial.o(i.USART1_IRQHandler) referenced from startup_stm32f10x_md.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(i.UsageFault_Handler) referenced from startup_stm32f10x_md.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_md.o(.text) referenced from startup_stm32f10x_md.o(RESET)
  - __main from __main.o(!!!main) referenced from startup_stm32f10x_md.o(.text)

  ### Global Symbols

  __main (Thumb, 8 bytes, Stack size 0 bytes, __main.o(!!!main))
  [Calls]

  - >> __scatterload
  - >> __rt_entry

  __scatterload (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter))
  [Called By]

  - >> __main

  __scatterload_rt2 (Thumb, 44 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)
  [Calls]

  - >> __rt_entry

  __scatterload_rt2_thumb_only (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __scatterload_null (Thumb, 0 bytes, Stack size unknown bytes, __scatter.o(!!!scatter), UNUSED)

  __decompress (Thumb, 58 bytes, Stack size unknown bytes, __dczerorl.o(!!dczerorl), UNUSED)

  __decompress0 (Thumb, 0 bytes, Stack size unknown bytes, __dczerorl.o(!!dczerorl), UNUSED)

  __scatterload_zeroinit (Thumb, 28 bytes, Stack size unknown bytes, __scatter_zi.o(!!handler_zi), UNUSED)

  __rt_lib_init (Thumb, 0 bytes, Stack size unknown bytes, libinit.o(.ARM.Collect$$libinit$$00000000))
  [Called By]

  - >> __rt_entry_li

  __rt_lib_init_alloca_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002E))

  __rt_lib_init_argv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000002C))

  __rt_lib_init_atexit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001B))

  __rt_lib_init_clock_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000021))

  __rt_lib_init_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000032))

  __rt_lib_init_exceptions_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000030))

  __rt_lib_init_fp_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000002))

  __rt_lib_init_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001F))

  __rt_lib_init_getenv_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000023))

  __rt_lib_init_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000A))

  __rt_lib_init_lc_collate_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000011))

  __rt_lib_init_lc_ctype_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000013))

  __rt_lib_init_lc_monetary_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000015))

  __rt_lib_init_lc_numeric_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000017))

  __rt_lib_init_lc_time_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000019))

  __rt_lib_init_preinit_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000004))

  __rt_lib_init_rand_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000E))

  __rt_lib_init_return (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000033))

  __rt_lib_init_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000001D))

  __rt_lib_init_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$00000025))

  __rt_lib_init_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libinit2.o(.ARM.Collect$$libinit$$0000000C))

  __rt_lib_shutdown (Thumb, 0 bytes, Stack size unknown bytes, libshutdown.o(.ARM.Collect$$libshutdown$$00000000))
  [Called By]

  - >> __rt_exit_ls

  __rt_lib_shutdown_cpp_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000004))

  __rt_lib_shutdown_fini_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000002))

  __rt_lib_shutdown_fp_trap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000009))

  __rt_lib_shutdown_heap_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000011))

  __rt_lib_shutdown_return (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000012))

  __rt_lib_shutdown_signal_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000C))

  __rt_lib_shutdown_stdio_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$00000006))

  __rt_lib_shutdown_user_alloc_1 (Thumb, 0 bytes, Stack size unknown bytes, libshutdown2.o(.ARM.Collect$$libshutdown$$0000000E))

  __rt_entry (Thumb, 0 bytes, Stack size unknown bytes, __rtentry.o(.ARM.Collect$$rtentry$$00000000))
  [Called By]

  - >> __scatterload_rt2
  - >> __main

  __rt_entry_presh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000002))

  __rt_entry_sh (Thumb, 0 bytes, Stack size unknown bytes, __rtentry4.o(.ARM.Collect$$rtentry$$00000004))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __rt_entry_sh ⇒ __user_setup_stackheap
  [Calls]
  - >> __user_setup_stackheap

  __rt_entry_li (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000A))
  [Calls]

  - >> __rt_lib_init

  __rt_entry_postsh_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$00000009))

  __rt_entry_main (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000D))
  [Stack]

  - Max Depth = 108 + Unknown Stack Size
  - Call Chain = __rt_entry_main ⇒ main ⇒ HC05_Init ⇒ Serial_Init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> main
  - >> exit

  __rt_entry_postli_1 (Thumb, 0 bytes, Stack size unknown bytes, __rtentry2.o(.ARM.Collect$$rtentry$$0000000C))

  __rt_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit.o(.ARM.Collect$$rtexit$$00000000))
  [Called By]

  - >> exit

  __rt_exit_ls (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000003))
  [Calls]

  - >> __rt_lib_shutdown

  __rt_exit_prels_1 (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000002))

  __rt_exit_exit (Thumb, 0 bytes, Stack size unknown bytes, rtexit2.o(.ARM.Collect$$rtexit$$00000004))
  [Calls]

  - >> _sys_exit

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_md.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  __user_initial_stackheap (Thumb, 0 bytes, Stack size unknown bytes, startup_stm32f10x_md.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  strcmp (Thumb, 128 bytes, Stack size 0 bytes, strcmpv7m.o(.text))
  [Called By]

  - >> main

  __use_two_region_memory (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_escrow$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __rt_heap_expand$2region (Thumb, 2 bytes, Stack size 0 bytes, heapauxi.o(.text), UNUSED)

  __user_setup_stackheap (Thumb, 74 bytes, Stack size 8 bytes, sys_stackheap_outer.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = __user_setup_stackheap
  [Calls]
  - >> __user_initial_stackheap
  - >> __user_perproc_libspace
  [Called By]
  - >> __rt_entry_sh

  exit (Thumb, 18 bytes, Stack size 8 bytes, exit.o(.text))
  [Stack]

  - Max Depth = 8 + Unknown Stack Size
  - Call Chain = exit
  [Calls]
  - >> __rt_exit
  [Called By]
  - >> __rt_entry_main

  __user_libspace (Thumb, 8 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  __user_perproc_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text))
  [Called By]

  - >> __user_setup_stackheap

  __user_perthread_libspace (Thumb, 0 bytes, Stack size 0 bytes, libspace.o(.text), UNUSED)

  _sys_exit (Thumb, 8 bytes, Stack size 0 bytes, sys_exit.o(.text))
  [Called By]

  - >> __rt_exit_exit

  __I$use$semihosting (Thumb, 0 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __use_no_semihosting_swi (Thumb, 2 bytes, Stack size 0 bytes, use_no_semi.o(.text), UNUSED)

  __semihosting_library_function (Thumb, 0 bytes, Stack size unknown bytes, indicate_semi.o(.text), UNUSED)

  Board_Timer_Flag_Get (Thumb, 22 bytes, Stack size 0 bytes, board_timer.o(i.Board_Timer_Flag_Get))
  [Called By]

  - >> main

  Board_Timer_Init (Thumb, 98 bytes, Stack size 24 bytes, board_timer.o(i.Board_Timer_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = Board_Timer_Init ⇒ NVIC_Init
  [Calls]
  - >> NVIC_Init
  - >> RCC_APB1PeriphClockCmd
  - >> TIM_TimeBaseInit
  - >> TIM_ITConfig
  - >> TIM_Cmd
  [Called By]
  - >> main

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  Delay_ms (Thumb, 24 bytes, Stack size 4 bytes, delay.o(i.Delay_ms))
  [Stack]

  - Max Depth = 4
  - Call Chain = Delay_ms
  [Calls]
  - >> Delay_us
  [Called By]
  - >> Delay_s

  Delay_s (Thumb, 24 bytes, Stack size 8 bytes, delay.o(i.Delay_s))
  [Stack]

  - Max Depth = 12
  - Call Chain = Delay_s ⇒ Delay_ms
  [Calls]
  - >> Delay_ms
  [Called By]
  - >> main

  Delay_us (Thumb, 46 bytes, Stack size 0 bytes, delay.o(i.Delay_us))
  [Called By]

  - >> NeZha_Delay_us
  - >> Delay_ms

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> Serial_Init
  - >> HC05_Init
  - >> NeZha_I2C_SdaDir
  - >> NeZha_I2C_Init
  - >> LED_Init

  GPIO_ReadOutputDataBit (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ReadOutputDataBit))
  [Called By]

  - >> LED1_Turn

  GPIO_WriteBit (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_WriteBit))
  [Called By]

  - >> NeZha_I2C_Stop
  - >> NeZha_I2C_Start
  - >> NeZha_I2C_SendByte
  - >> NeZha_I2C_Init

  HC05_GetData (Thumb, 50 bytes, Stack size 16 bytes, hc05.o(i.HC05_GetData))
  [Stack]

  - Max Depth = 16
  - Call Chain = HC05_GetData
  [Calls]
  - >> Serial_GetRxFlag
  - >> Serial_GetRxData
  [Called By]
  - >> main

  HC05_Init (Thumb, 42 bytes, Stack size 8 bytes, hc05.o(i.HC05_Init))
  [Stack]

  - Max Depth = 108
  - Call Chain = HC05_Init ⇒ Serial_Init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> Serial_Init
  [Called By]
  - >> main

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  LED1_Turn (Thumb, 30 bytes, Stack size 8 bytes, led.o(i.LED1_Turn))
  [Stack]

  - Max Depth = 8
  - Call Chain = LED1_Turn
  [Calls]
  - >> GPIO_ReadOutputDataBit
  [Called By]
  - >> main

  LED_Init (Thumb, 40 bytes, Stack size 8 bytes, led.o(i.LED_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = LED_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> Serial_Init
  - >> Board_Timer_Init

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> main
  - >> Serial_Init

  NeZha_Delay_ms (Thumb, 24 bytes, Stack size 16 bytes, nezha_i2c.o(i.NeZha_Delay_ms))
  [Stack]

  - Max Depth = 24
  - Call Chain = NeZha_Delay_ms ⇒ NeZha_Delay_us
  [Calls]
  - >> NeZha_Delay_us
  [Called By]
  - >> NeZha_I2C_Init
  - >> NeZha_Reset

  NeZha_Delay_us (Thumb, 12 bytes, Stack size 8 bytes, nezha_i2c.o(i.NeZha_Delay_us))
  [Stack]

  - Max Depth = 8
  - Call Chain = NeZha_Delay_us
  [Calls]
  - >> Delay_us
  [Called By]
  - >> NeZha_I2C_Stop
  - >> NeZha_I2C_Start
  - >> NeZha_I2C_SendByte
  - >> NeZha_Delay_ms

  NeZha_I2C_Init (Thumb, 80 bytes, Stack size 8 bytes, nezha_i2c.o(i.NeZha_I2C_Init))
  [Stack]

  - Max Depth = 32
  - Call Chain = NeZha_I2C_Init ⇒ GPIO_Init
  [Calls]
  - >> GPIO_WriteBit
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> NeZha_Delay_ms
  [Called By]
  - >> NeZha_Init

  NeZha_I2C_SdaDir (Thumb, 50 bytes, Stack size 16 bytes, nezha_i2c.o(i.NeZha_I2C_SdaDir))
  [Stack]

  - Max Depth = 40
  - Call Chain = NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  [Called By]
  - >> NeZha_I2C_SendByte

  NeZha_I2C_SendByte (Thumb, 120 bytes, Stack size 16 bytes, nezha_i2c.o(i.NeZha_I2C_SendByte))
  [Stack]

  - Max Depth = 56
  - Call Chain = NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> GPIO_WriteBit
  - >> NeZha_I2C_SdaDir
  - >> NeZha_Delay_us
  [Called By]
  - >> NeZha_WriteCommand
  - >> NeZha_Motor4_SetPwm
  - >> NeZha_Motor3_SetPwm
  - >> NeZha_Motor2_SetPwm
  - >> NeZha_Motor1_SetPwm

  NeZha_I2C_Start (Thumb, 50 bytes, Stack size 8 bytes, nezha_i2c.o(i.NeZha_I2C_Start))
  [Stack]

  - Max Depth = 16
  - Call Chain = NeZha_I2C_Start ⇒ NeZha_Delay_us
  [Calls]
  - >> GPIO_WriteBit
  - >> NeZha_Delay_us
  [Called By]
  - >> NeZha_WriteCommand
  - >> NeZha_Motor4_SetPwm
  - >> NeZha_Motor3_SetPwm
  - >> NeZha_Motor2_SetPwm
  - >> NeZha_Motor1_SetPwm

  NeZha_I2C_Stop (Thumb, 40 bytes, Stack size 8 bytes, nezha_i2c.o(i.NeZha_I2C_Stop))
  [Stack]

  - Max Depth = 16
  - Call Chain = NeZha_I2C_Stop ⇒ NeZha_Delay_us
  [Calls]
  - >> GPIO_WriteBit
  - >> NeZha_Delay_us
  [Called By]
  - >> NeZha_WriteCommand
  - >> NeZha_Motor4_SetPwm
  - >> NeZha_Motor3_SetPwm
  - >> NeZha_Motor2_SetPwm
  - >> NeZha_Motor1_SetPwm

  NeZha_Init (Thumb, 12 bytes, Stack size 8 bytes, nezha.o(i.NeZha_Init))
  [Stack]

  - Max Depth = 80
  - Call Chain = NeZha_Init ⇒ NeZha_Reset ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_I2C_Init
  - >> NeZha_Reset
  [Called By]
  - >> main

  NeZha_Motor1_SetPwm (Thumb, 74 bytes, Stack size 32 bytes, nezha.o(i.NeZha_Motor1_SetPwm))
  [Stack]

  - Max Depth = 96
  - Call Chain = NeZha_Motor1_SetPwm ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_I2C_Stop
  - >> NeZha_I2C_Start
  - >> NeZha_I2C_SendByte
  - >> NeZha_WriteCommand
  [Called By]
  - >> main

  NeZha_Motor2_SetPwm (Thumb, 74 bytes, Stack size 32 bytes, nezha.o(i.NeZha_Motor2_SetPwm))
  [Stack]

  - Max Depth = 96
  - Call Chain = NeZha_Motor2_SetPwm ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_I2C_Stop
  - >> NeZha_I2C_Start
  - >> NeZha_I2C_SendByte
  - >> NeZha_WriteCommand
  [Called By]
  - >> main

  NeZha_Motor3_SetPwm (Thumb, 74 bytes, Stack size 32 bytes, nezha.o(i.NeZha_Motor3_SetPwm))
  [Stack]

  - Max Depth = 96
  - Call Chain = NeZha_Motor3_SetPwm ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_I2C_Stop
  - >> NeZha_I2C_Start
  - >> NeZha_I2C_SendByte
  - >> NeZha_WriteCommand
  [Called By]
  - >> main

  NeZha_Motor4_SetPwm (Thumb, 74 bytes, Stack size 32 bytes, nezha.o(i.NeZha_Motor4_SetPwm))
  [Stack]

  - Max Depth = 96
  - Call Chain = NeZha_Motor4_SetPwm ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_I2C_Stop
  - >> NeZha_I2C_Start
  - >> NeZha_I2C_SendByte
  - >> NeZha_WriteCommand
  [Called By]
  - >> main

  NeZha_Motor_Init (Thumb, 10 bytes, Stack size 8 bytes, nezha.o(i.NeZha_Motor_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = NeZha_Motor_Init ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_WriteCommand
  [Called By]
  - >> main

  NeZha_Reset (Thumb, 16 bytes, Stack size 8 bytes, nezha.o(i.NeZha_Reset))
  [Stack]

  - Max Depth = 72
  - Call Chain = NeZha_Reset ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_Delay_ms
  - >> NeZha_WriteCommand
  [Called By]
  - >> NeZha_Init

  NeZha_TailLeftLed_Turn (Thumb, 10 bytes, Stack size 8 bytes, nezha.o(i.NeZha_TailLeftLed_Turn))
  [Stack]

  - Max Depth = 72
  - Call Chain = NeZha_TailLeftLed_Turn ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_WriteCommand
  [Called By]
  - >> main

  NeZha_TailLeftLed_TurnOff (Thumb, 10 bytes, Stack size 8 bytes, nezha.o(i.NeZha_TailLeftLed_TurnOff))
  [Stack]

  - Max Depth = 72
  - Call Chain = NeZha_TailLeftLed_TurnOff ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_WriteCommand
  [Called By]
  - >> main

  NeZha_TailLeftLed_TurnOn (Thumb, 10 bytes, Stack size 8 bytes, nezha.o(i.NeZha_TailLeftLed_TurnOn))
  [Stack]

  - Max Depth = 72
  - Call Chain = NeZha_TailLeftLed_TurnOn ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_WriteCommand
  [Called By]
  - >> main

  NeZha_TailRightLed_Turn (Thumb, 10 bytes, Stack size 8 bytes, nezha.o(i.NeZha_TailRightLed_Turn))
  [Stack]

  - Max Depth = 72
  - Call Chain = NeZha_TailRightLed_Turn ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_WriteCommand
  [Called By]
  - >> main

  NeZha_TailRightLed_TurnOff (Thumb, 10 bytes, Stack size 8 bytes, nezha.o(i.NeZha_TailRightLed_TurnOff))
  [Stack]

  - Max Depth = 72
  - Call Chain = NeZha_TailRightLed_TurnOff ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_WriteCommand
  [Called By]
  - >> main

  NeZha_TailRightLed_TurnOn (Thumb, 10 bytes, Stack size 8 bytes, nezha.o(i.NeZha_TailRightLed_TurnOn))
  [Stack]

  - Max Depth = 72
  - Call Chain = NeZha_TailRightLed_TurnOn ⇒ NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_WriteCommand
  [Called By]
  - >> main

  NeZha_WriteCommand (Thumb, 32 bytes, Stack size 8 bytes, nezha.o(i.NeZha_WriteCommand))
  [Stack]

  - Max Depth = 64
  - Call Chain = NeZha_WriteCommand ⇒ NeZha_I2C_SendByte ⇒ NeZha_I2C_SdaDir ⇒ GPIO_Init
  [Calls]
  - >> NeZha_I2C_Stop
  - >> NeZha_I2C_Start
  - >> NeZha_I2C_SendByte
  [Called By]
  - >> NeZha_TailRightLed_TurnOn
  - >> NeZha_TailRightLed_TurnOff
  - >> NeZha_TailRightLed_Turn
  - >> NeZha_TailLeftLed_TurnOn
  - >> NeZha_TailLeftLed_TurnOff
  - >> NeZha_TailLeftLed_Turn
  - >> NeZha_Reset
  - >> NeZha_Motor_Init
  - >> NeZha_Motor4_SetPwm
  - >> NeZha_Motor3_SetPwm
  - >> NeZha_Motor2_SetPwm
  - >> NeZha_Motor1_SetPwm

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> Board_Timer_Init

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> Serial_Init
  - >> HC05_Init
  - >> NeZha_I2C_SdaDir
  - >> NeZha_I2C_Init
  - >> LED_Init

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  Serial_GetRxData (Thumb, 6 bytes, Stack size 0 bytes, serial.o(i.Serial_GetRxData))
  [Called By]

  - >> HC05_GetData

  Serial_GetRxFlag (Thumb, 22 bytes, Stack size 0 bytes, serial.o(i.Serial_GetRxFlag))
  [Called By]

  - >> HC05_GetData

  Serial_Init (Thumb, 174 bytes, Stack size 32 bytes, serial.o(i.Serial_Init))
  [Stack]

  - Max Depth = 100
  - Call Chain = Serial_Init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> NVIC_PriorityGroupConfig
  - >> NVIC_Init
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_Cmd
  [Called By]
  - >> HC05_Init

  Serial_SendByte (Thumb, 28 bytes, Stack size 8 bytes, serial.o(i.Serial_SendByte))
  [Stack]

  - Max Depth = 8
  - Call Chain = Serial_SendByte
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Called By]
  - >> USART1_IRQHandler

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SystemInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(.text)

  TIM2_IRQHandler (Thumb, 28 bytes, Stack size 8 bytes, board_timer.o(i.TIM2_IRQHandler))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM2_IRQHandler ⇒ TIM_GetITStatus
  [Calls]
  - >> TIM_GetITStatus
  - >> TIM_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  TIM_ClearITPendingBit (Thumb, 6 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_ClearITPendingBit))
  [Called By]

  - >> TIM2_IRQHandler

  TIM_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_Cmd))
  [Called By]

  - >> Board_Timer_Init

  TIM_GetITStatus (Thumb, 34 bytes, Stack size 12 bytes, stm32f10x_tim.o(i.TIM_GetITStatus))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_GetITStatus
  [Called By]
  - >> TIM2_IRQHandler

  TIM_ITConfig (Thumb, 18 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_ITConfig))
  [Called By]

  - >> Board_Timer_Init

  TIM_TimeBaseInit (Thumb, 122 bytes, Stack size 0 bytes, stm32f10x_tim.o(i.TIM_TimeBaseInit))
  [Called By]

  - >> Board_Timer_Init

  USART1_IRQHandler (Thumb, 52 bytes, Stack size 8 bytes, serial.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> Serial_SendByte
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  - >> USART_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_md.o(RESET)

  USART_ClearITPendingBit (Thumb, 30 bytes, Stack size 8 bytes, stm32f10x_usart.o(i.USART_ClearITPendingBit))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_ClearITPendingBit
  [Called By]
  - >> USART1_IRQHandler

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
  [Called By]

  - >> Serial_Init

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> Serial_SendByte

  USART_GetITStatus (Thumb, 84 bytes, Stack size 16 bytes, stm32f10x_usart.o(i.USART_GetITStatus))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f10x_usart.o(i.USART_ITConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> Serial_Init

  USART_Init (Thumb, 210 bytes, Stack size 56 bytes, stm32f10x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> Serial_Init

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_ReceiveData))
  [Called By]

  - >> USART1_IRQHandler

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
  [Called By]

  - >> Serial_SendByte

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_md.o(RESET)

  main (Thumb, 968 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 108
  - Call Chain = main ⇒ HC05_Init ⇒ Serial_Init ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> NVIC_PriorityGroupConfig
  - >> HC05_Init
  - >> HC05_GetData
  - >> NeZha_TailRightLed_TurnOn
  - >> NeZha_TailRightLed_TurnOff
  - >> NeZha_TailRightLed_Turn
  - >> NeZha_TailLeftLed_TurnOn
  - >> NeZha_TailLeftLed_TurnOff
  - >> NeZha_TailLeftLed_Turn
  - >> NeZha_Motor_Init
  - >> NeZha_Motor4_SetPwm
  - >> NeZha_Motor3_SetPwm
  - >> NeZha_Motor2_SetPwm
  - >> NeZha_Motor1_SetPwm
  - >> NeZha_Init
  - >> Board_Timer_Init
  - >> Board_Timer_Flag_Get
  - >> LED_Init
  - >> LED1_Turn
  - >> Delay_s
  - >> strcmp
  [Called By]
  - >> __rt_entry_main

  ### Local Symbols

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SetSysClock))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_stm32f10x.o(i.SetSysClockTo72))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  ### Undefined Global Symbols